1. In Eagle, use DRC > Masks to set Cream min to 5.5 mil and max to 7mil.Make sure this actually adjusts cream field sizes! The comparator footprint in the TI library is wronnggggg, for example
2. Export to gerber file using standard procedure and print to Full Spectrum driver
3. Power settings for parchment paper stencil are vector speed 80%, power 0.2%, vector current 20%
4. Cut as a vector